

Ironmongery Specification



Product : ZDC0024

Description : Universal Door Closer Adjustable Power Size 2-4

Finish : Satin Stainless Steel Body & Arm

Testing : BS EN1154, CE Marked & Certifire Approved in Size 3



Product : ZDC003

Description : Fixed Power Size 3 Door Closer

Finish : Silver Enamel Body & Arm

Testing : BS EN1154, CE Marked & Certifire Approved in Size 3



Product : 794SHU

Description : 180 Degree door Viewer

Finish : Satin Chrome Plated

[](http://www.google.co.uk/url?sa=i&rct=j&q=&esrc=s&frm=1&source=images&cd=&cad=rja&uact=8&ved=0CAcQjRxqFQoTCKP1-bGS78YCFYFu2wod3poH7A&url=http://luxuryhandles.co.uk/din-locks/zoo-din-radius-escape-lock-zdl7260escr.html&ei=zsKvVaPWCoHd7QbetZ7gDg&bvm=bv.98197061,d.ZGU&psig=AFQjCNFZOj_WrDAUJL_UE3pN27hRya5Oww&ust=1437668428004834)

Product : ZDL7260R

Description : Euro-Profile Din Standard Mortice Sash Lock 60mm Backset, 72mm Centres

Finish : Satin Stainless Steel Faceplate & Strike

Testing : BS EN12209 : 2003 Grade 3, CE Marked & Certifire Approved




Product : ZDL0060R

Description : Euro-Profile Din Standard Mortice Deadlock , 60mm Backset

Finish : Satin Stainless Steel Faceplate & Strike

Testing : BS EN12209 Grade 3, CE Marked & Certifire Approved



Product : V10EP70CT

Description : Euro-Profile Cylinder & Turn Under master key & Construction Keyed

Finish : Satin Chrome Plated

Testing : BS-EN1303 Security Grade 2 Restricted 10 pin cylinder



Product : ZAS16SS

Description : Euro Profile Cylinder Pull

Finish : Grade 304 Satin Stainless Steel



Product : ZTLA76R

Description : 76mm Heavy Duty Tubular Latch Radius Forend

Finish : Grade 304 Satin Stainless Steel



Product : ZTDA76R

Description : 76mm Heavy Duty Tubular Deadbolt Radius Forend

Finish : Grade 304 Satin Stainless Steel



Product : ZCS160SS

Description : 19mm Lever on 52x8mm Sprung Rose

Finish : Grade 304 Satin Stainless Steel

Testing : BS EN1906 Grade 3



Product : OV6B/319SSS

Description : 300x19mm Pull Handle Bolt Through Fixing

Finish : Grade 304 Satin Stainless Steel

Testing : BS EN1634-1



Product : TTFP338SS

Description : 330x75x1.5mm Finger Plate c/w Radius Corners

Finish : Grade 304 Satin Stainless Steel



Product : ZCS001

Description : Euro-Profile Cylinder Escutcheon 52x8mm


Finish : Grade 304 Satin Stainless Steel



Product : ZCS004

Description : Bathroom Thumbturn & Emergency Release c/e Indicator 52x8mm

Finish : Grade 304 Satin Stainless Steel



[](http://www.zoohardware.co.uk/Products/158/ZAS14-Dust-Socket-Concrete.html)

Product : SHP/1003/150/SC

Description : 150x25mm Necked Barrel Bolt

Finish : Satin Chrome Plate

Product : ZAS14SSS

Description : Dust Excluding Socket

Finish : Satin Stainless Steel



Product : TT606SS

Description : 75mm Dia Sign to Read “Fire Door Keep Shut”

Finish : Satin Stainless Steel

Testing : BS 5499-4



Product : TT605SS

Description : 75mm Dia Sign to Read “Fire Door Keep Locked”

Finish : Satin Stainless Steel

Testing : BS 5499-4

[](http://www.bing.com/images/search?q=kicking+plate&id=C23BD470C7E3685DB877BE25EFCD14A9218930C3&FORM=IQFRBA)

Product : AJC900X150SSS

Description : Kicking Plate 150mm High

Finish : Grade 304 Satin Stainless Steel

Notes : Size Specified is Nominal, Exact Site Sizes Required